{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["Sheet0"],"not_rendered":{"external_links":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet0","index":0,"n_rows":5,"n_cols":9,"rows_kept":5,"flags":["formulas_cached_only"]}
["信息类别","首页推荐","标题","上传图片","内容","创建时间","SEO标题","SEO关键字","SEO描述"]
[54,false,"T23",null,"<p>\n<p>主要特性</p>\n<p>输入电压：24~220VDC</p>\n<p>额定电流：1~2A</p>\n<p>行程：100~350mm</p>\n<p>推力：1000~3000N</p>\n<p>速度：5~15mm/s</p>\n</p>"]
[54,false,"T34",null,"<p>\n<p>主要特性</p>\n<p>输入电压：24~220VDC</p>\n<p>额定电流：1~2A</p>\n<p>行程：150~350mm</p>\n<p>推力：1000~6000N</p>\n<p>速度：5~15mm/s</p>\n</p>"]
[54,false,"T41",null,"<p>\n<p>主要特性</p>\n<p>输入电压：24VDC</p>\n<p>额定电流：3.5A</p>\n<p>行程：150~350mm</p>\n<p>推力：3000~3000N</p>\n<p>速度：5~15mm/s</p>\n</p>"]
[54,false,"T44",null,"<p>\n<p>主要特性</p>\n<p>输入电压：24VDC</p>\n<p>额定电流：3.5A</p>\n<p>行程：100~350mm</p>\n<p>推力：3000~3000N</p>\n<p>速度：5~15mm/s</p>\n</p>"]